1. Load hyperspectral
   1. MESMA using SVD in database
2. Load Lidar as point cloud
   1. Use spark to create DSM and DHM and then CHM
   2. Use spark to do watershed
   3. Use Spark and rules to enhance MESMA outputs